The DreamCE.vcw workspace is for the Windows CE projects and should
 be loaded in the eMbedded Visual Toolkit.

The DreamNT.dsw workspace is for the Windows NT projects and 
should be loaded in Microsoft Visual C++ 6.0.

The ouput binaries can be found in the Target directory for 
each processor type. 

In order for the CELoader sample to be executed, you will need 
to have the IP.bin, 1st_read.bin or 0winceos.bin files and WinCE
 directory that can be found in distributions of Boob!Boy, GypPlay,
 and DCMp3. 

Copy the CELoader.exe and DUiMan.dll files, along with the files 
and directories mentioned above to root directory of the target 
CD. In addition, because programs are typically started via a registry
 entry in the distributed firmware, you will need to rename the 
CELoader.exe file to same file name that the other program was using. 

CELoader also makes use of the Arial True Type Font, so make 
sure that an Arial.ttf file is in the WinCE directory.