The DreamCE.vcw workspace is for the Windows CE projects and should be
 loaded in the eMbedded Visual Toolkit.

The DreamNT.dsw workspace is for the Windows NT projects and 
should be loaded in Microsoft Visual C++ 6.0.

The ouput binaries can be found in the Target directory 
for each processor type. 

In order for the CELoader sample to be executed, you 
will need to have the IP.bin, 1st_read.bin or 0winceos.bin 
files and WinCE directory that can be found in distributions 
of Boob!Boy, GypPlay, and DCMp3. 

Copy the CELoader.exe and DUiMan.dll files, along with the
 files and directories mentioned above to root directory of
 the target CD. In addition, because programs are typically 
started via a registry entry in the distributed firmware, you
 will need to rename the CELoader.exe file to same file name
 that the other program was using. 

CELoader also makes use of the Arial True Type
 Font, so make sure that an Arial.ttf file is in 
the WinCE directory.